

# N1




Defining a new TASKORG C2IP should automatically adding it to the current Mission C2IP Explorer

# N2




Defining a new C2IP should automaticaly generate and ADD a new C2IE of the same type

# N3



Creating a new C2IP from the C2IP Explorer of the Mission should automatically add the newly C2IP to the C2IP Explorer of the Mission.

# N4



Adding a new BSO to a destination TASKORG C2IP duplicates the view with all C2IEs where the BSO is already part of